IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2026-07-05T18:53:46"
Preprocessor: "IfcOpenShell 0.8.4-e8eb5e4"
Originating system: "IfcOpenShell 0.8.4-e8eb5e4"
Application: "ifcopenshell script" version "0.8.4" identifier "AIRS BIM generator" by Organization "AIRS (Ventar-S)" description "AIRS modern climate systems"

People and organizations
  Person "AIRS" "Ventar-S" of Organization "AIRS (Ventar-S)" description "AIRS modern climate systems"
  Owner history of Person "AIRS" "Ventar-S" of Organization "AIRS (Ventar-S)" description "AIRS modern climate systems" | application "ifcopenshell script" version "0.8.4" identifier "AIRS BIM generator" by Organization "AIRS (Ventar-S)" description "AIRS modern climate systems" | change ADDED | created 1783266826 (2026-07-05T15:53:46Z) | last modified 1783266826 (2026-07-05T15:53:46Z) by Person "AIRS" "Ventar-S" of Organization "AIRS (Ventar-S)" description "AIRS modern climate systems" with "ifcopenshell script" version "0.8.4" identifier "AIRS BIM generator" by Organization "AIRS (Ventar-S)" description "AIRS modern climate systems"

Units
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND
  MASSUNIT: KILO GRAM

Spatial structure
IFCPROJECT "AIRS-AIRS-TS-BIM"
  IFCSITE "Site"
    IFCBUILDING "Building"
      IFCBUILDINGSTOREY "Storey" | elevation 0.
        contains 1 element
          1 x IFCSENSOR | type IFCSENSORTYPE "AIRS TS" | FIRESENSOR | names: "AIRS TS" | descriptions: "Терморазмыкающее устройство (ТРУ) для перевода противопожарного клапана в охранное положение при превышении порога температуры" | material: "Пластик, металлический зонд" | property sets: Pset_ManufacturerTypeInformation, Pset_AIRS_ThermalCutoff

Types
  IFCSENSORTYPE "AIRS TS" | element type "AIRS-TS" | FIRESENSOR | 1 occurrence | description "Терморазмыкающее устройство (ТРУ) для перевода противопожарного клапана в охранное положение при превышении порога температуры"

Property sets
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCSENSOR)
    Manufacturer = "AIRS (ООО ТД Вентар-С)" (IFCTEXT)
    ModelLabel = "AIRS TS" (IFCTEXT)
    ModelReference = "AIRS-TS" (IFCTEXT)
    ProductionYear = 2026 (IFCINTEGER)
  Pset_AIRS_ThermalCutoff | properties | on 1 object (1 IFCSENSOR)
    AmbientHumidity = "5-95% RH, без образования конденсата" (IFCTEXT)
    AmbientTemperatureRange_C = "-30..+120" (IFCTEXT)
    IngressProtection = "IP54" (IFCTEXT)
    Maintenance = "кнопка ручной проверки работоспособности" (IFCTEXT)
    Standards = "CE / RoHS / EAC / ISO" (IFCTEXT)
    StorageTemperatureRange_C = "-30..+120" (IFCTEXT)
    TripThreshold_C = 72 (IFCINTEGER)
    Voltage = "24 В AC/DC / 230 В AC +-10%" (IFCTEXT)
    Weight_kg = 0.1 (IFCREAL)