IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2026-07-05T23:59:56"
Preprocessor: "IfcOpenShell 0.8.4-e8eb5e4"
Originating system: "IfcOpenShell 0.8.4-e8eb5e4"
Application: "ifcopenshell script" version "0.8.4" identifier "AIRS BIM generator" by Organization "AIRS (Ventar-S)" description "AIRS modern climate systems"

People and organizations
  Person "AIRS" "Ventar-S" of Organization "AIRS (Ventar-S)" description "AIRS modern climate systems"
  Owner history of Person "AIRS" "Ventar-S" of Organization "AIRS (Ventar-S)" description "AIRS modern climate systems" | application "ifcopenshell script" version "0.8.4" identifier "AIRS BIM generator" by Organization "AIRS (Ventar-S)" description "AIRS modern climate systems" | change ADDED | created 1783285196 (2026-07-05T20:59:56Z) | last modified 1783285196 (2026-07-05T20:59:56Z) by Person "AIRS" "Ventar-S" of Organization "AIRS (Ventar-S)" description "AIRS modern climate systems" with "ifcopenshell script" version "0.8.4" identifier "AIRS BIM generator" by Organization "AIRS (Ventar-S)" description "AIRS modern climate systems"

Units
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND
  MASSUNIT: KILO GRAM

Spatial structure
IFCPROJECT "AIRS-KPD-DU-S-BIM"
  IFCSITE "Site"
    IFCBUILDING "Building"
      IFCBUILDINGSTOREY "Storey" | elevation 0.
        contains 1 element
          1 x IFCDAMPER | type IFCDAMPERTYPE "AIRS КПД-ДУ (стеновой)" | FIRESMOKEDAMPER | names: "AIRS КПД-ДУ (стеновой)" | descriptions: "Клапан дымовой противопожарный КПД-ДУ, стеновое исполнение" | material: "Оцинкованная сталь 1 мм" | property sets: Pset_ManufacturerTypeInformation, Pset_AIRS_FireDamper

Types
  IFCDAMPERTYPE "AIRS КПД-ДУ (стеновой)" | element type "KPD-DU-S" | FIRESMOKEDAMPER | 1 occurrence | description "Клапан дымовой противопожарный КПД-ДУ, стеновое исполнение"

Property sets
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDAMPER)
    Manufacturer = "AIRS (ООО ТД Вентар-С)" (IFCTEXT)
    ModelLabel = "AIRS КПД-ДУ (стеновой)" (IFCTEXT)
    ModelReference = "KPD-DU-S" (IFCTEXT)
    ProductionYear = 2026 (IFCINTEGER)
  Pset_AIRS_FireDamper | properties | on 1 object (1 IFCDAMPER)
    ActuatorOptions = "BELIMO/AIRS реверсивный, BELIMO/AIRS с возвратной пружиной, электромагнитный" (IFCTEXT)
    ActuatorVoltage = "220/24 В" (IFCTEXT)
    Application = "Клапан дымоудаления (приточно-вытяжная противодымная вентиляция)" (IFCTEXT)
    BodyDepth_mm = 205. (IFCREAL)
    BodyMaterial = "Оцинкованная/нержавеющая сталь 1 мм" (IFCTEXT)
    FireResistanceRating = "EI 90 / EI 120" (IFCTEXT)
    FlangeWidth_mm = 45. (IFCREAL)
    NominalSize_AxB_mm = "500x300 (пример типоразмера, изготавливается по размеру заказчика)" (IFCTEXT)
    Series = "КПД-ДУ (стеновой)" (IFCTEXT)
    Standards = "EI 90 / EI 120, соответствует ГОСТ Р 53301, ТР ТС 004/2011, 020/2011" (IFCTEXT)