IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2026-07-05T18:53:46"
Preprocessor: "IfcOpenShell 0.8.4-e8eb5e4"
Originating system: "IfcOpenShell 0.8.4-e8eb5e4"
Application: "ifcopenshell script" version "0.8.4" identifier "AIRS BIM generator" by Organization "AIRS (Ventar-S)" description "AIRS modern climate systems"

People and organizations
  Person "AIRS" "Ventar-S" of Organization "AIRS (Ventar-S)" description "AIRS modern climate systems"
  Owner history of Person "AIRS" "Ventar-S" of Organization "AIRS (Ventar-S)" description "AIRS modern climate systems" | application "ifcopenshell script" version "0.8.4" identifier "AIRS BIM generator" by Organization "AIRS (Ventar-S)" description "AIRS modern climate systems" | change ADDED | created 1783266826 (2026-07-05T15:53:46Z) | last modified 1783266826 (2026-07-05T15:53:46Z) by Person "AIRS" "Ventar-S" of Organization "AIRS (Ventar-S)" description "AIRS modern climate systems" with "ifcopenshell script" version "0.8.4" identifier "AIRS BIM generator" by Organization "AIRS (Ventar-S)" description "AIRS modern climate systems"

Units
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND
  MASSUNIT: KILO GRAM

Spatial structure
IFCPROJECT "AIRS-VAV-LMV24-SR-BIM"
  IFCSITE "Site"
    IFCBUILDING "Building"
      IFCBUILDINGSTOREY "Storey" | elevation 0.
        contains 1 element
          1 x IFCACTUATOR | type IFCACTUATORTYPE "AIRS VAV-LMV24-SR" | ELECTRICACTUATOR | names: "AIRS VAV-LMV24-SR" | descriptions: "Электропривод воздушной заслонки переменного объёма, Modbus RTU / 0-10В, 6 Нм, 24В DC (серия VAV-LMV-SR)" | material: "Steel + ABS plastic housing" | property sets: Pset_ManufacturerTypeInformation, Pset_AIRS_VAVActuator

Types
  IFCACTUATORTYPE "AIRS VAV-LMV24-SR" | element type "VAV-LMV24-SR" | ELECTRICACTUATOR | 1 occurrence | description "Электропривод воздушной заслонки переменного объёма, Modbus RTU / 0-10В, 6 Нм, 24В DC (серия VAV-LMV-SR)"

Property sets
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCACTUATOR)
    Manufacturer = "AIRS (ООО ТД Вентар-С)" (IFCTEXT)
    ModelLabel = "AIRS VAV-LMV24-SR" (IFCTEXT)
    ModelReference = "VAV-LMV24-SR" (IFCTEXT)
    ProductionYear = 2026 (IFCINTEGER)
  Pset_AIRS_VAVActuator | properties | on 1 object (1 IFCACTUATOR)
    AmbientTemperatureRange_C = "0..+50" (IFCTEXT)
    AnalogInputs = "NTC 10кОм датчик температуры; датчик давления 0-900 Па" (IFCTEXT)
    AuxiliarySwitches = "2xSPDT, 3(1,5)A, AC 250V" (IFCTEXT)
    Communication = "RS-485 (полудуплекс), Modbus RTU, до 1125 м" (IFCTEXT)
    ControlSignalType = "0(2)-10В / 0(4)-20мА DC, RS-485 Modbus RTU" (IFCTEXT)
    ControlType = "2х/3х-позиционное, RS-485 Modbus RTU" (IFCTEXT)
    FeedbackSignalType = "0-10В / 4-20мА DC" (IFCTEXT)
    IngressProtection = "IP44" (IFCTEXT)
    MaxDamperArea_m2 = 1.5 (IFCREAL)
    MountingShaftRound_mm = "10-20" (IFCTEXT)
    MountingShaftSquare_mm = "10-16" (IFCTEXT)
    PowerConsumptionIdle_W = 0.5 (IFCREAL)
    PowerConsumptionRunning_W = 4.5 (IFCREAL)
    ProtectionClass = "III" (IFCTEXT)
    RatedPower_VA = 3. (IFCREAL)
    RatedTorque_Nm = 6. (IFCREAL)
    RotationAngle_deg = "0-90" (IFCTEXT)
    RunningTime_s = 30 (IFCINTEGER)
    Series = "VAV-LMV-SR" (IFCTEXT)
    ServiceLife_cycles = 60000 (IFCINTEGER)
    Standards = "CE / RoHS / EAC / ISO" (IFCTEXT)
    StorageTemperatureRange_C = "-30..+65" (IFCTEXT)
    Voltage = "24 В DC" (IFCTEXT)
    Weight_kg = 0.75 (IFCREAL)