IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2026-07-05T18:53:46"
Preprocessor: "IfcOpenShell 0.8.4-e8eb5e4"
Originating system: "IfcOpenShell 0.8.4-e8eb5e4"
Application: "ifcopenshell script" version "0.8.4" identifier "AIRS BIM generator" by Organization "AIRS (Ventar-S)" description "AIRS modern climate systems"

People and organizations
  Person "AIRS" "Ventar-S" of Organization "AIRS (Ventar-S)" description "AIRS modern climate systems"
  Owner history of Person "AIRS" "Ventar-S" of Organization "AIRS (Ventar-S)" description "AIRS modern climate systems" | application "ifcopenshell script" version "0.8.4" identifier "AIRS BIM generator" by Organization "AIRS (Ventar-S)" description "AIRS modern climate systems" | change ADDED | created 1783266826 (2026-07-05T15:53:46Z) | last modified 1783266826 (2026-07-05T15:53:46Z) by Person "AIRS" "Ventar-S" of Organization "AIRS (Ventar-S)" description "AIRS modern climate systems" with "ifcopenshell script" version "0.8.4" identifier "AIRS BIM generator" by Organization "AIRS (Ventar-S)" description "AIRS modern climate systems"

Units
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND
  MASSUNIT: KILO GRAM

Spatial structure
IFCPROJECT "AIRS-AIRS-AVT-230-BIM"
  IFCSITE "Site"
    IFCBUILDING "Building"
      IFCBUILDINGSTOREY "Storey" | elevation 0.
        contains 1 element
          1 x IFCCONTROLLER | type IFCCONTROLLERTYPE "AIRS AVT 230" | MULTIPOSITION | names: "AIRS AVT 230" | descriptions: "Блок управления положением заслонки (реверсивного электропривода) с пультом дистанционного управления" | material: "Пластиковый корпус" | property sets: Pset_ManufacturerTypeInformation, Pset_AIRS_PositionController

Types
  IFCCONTROLLERTYPE "AIRS AVT 230" | element type "AIRS-AVT-230" | MULTIPOSITION | 1 occurrence | description "Блок управления положением заслонки (реверсивного электропривода) с пультом дистанционного управления"

Property sets
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCCONTROLLER)
    Manufacturer = "AIRS (ООО ТД Вентар-С)" (IFCTEXT)
    ModelLabel = "AIRS AVT 230" (IFCTEXT)
    ModelReference = "AIRS-AVT-230" (IFCTEXT)
    ProductionYear = 2026 (IFCINTEGER)
  Pset_AIRS_PositionController | properties | on 1 object (1 IFCCONTROLLER)
    AmbientTemperatureRange_C = "-30..+50" (IFCTEXT)
    ControlType = "Ручное и дистанционное" (IFCTEXT)
    IngressProtection = "IP44" (IFCTEXT)
    MaxPower_W = 300. (IFCREAL)
    PeakOutputCurrent_A = 3. (IFCREAL)
    PositionIndication = "цифровой экран" (IFCTEXT)
    PresetAngles_deg = "0,18,36,54,72,90" (IFCTEXT)
    PresetPositions = 6 (IFCINTEGER)
    ProtectionClass = "II" (IFCTEXT)
    RemoteFrequency_MHz = 315. (IFCREAL)
    RemoteRange_m = 100 (IFCINTEGER)
    ServiceLife_cycles = 60000 (IFCINTEGER)
    Standards = "CE / RoHS / EAC / ISO" (IFCTEXT)
    StorageTemperatureRange_C = "-30..+70" (IFCTEXT)
    Voltage = "230 В AC +-10%" (IFCTEXT)
    Weight_kg = 0.1 (IFCREAL)